Head for High Temperature Applications

|  |  |
| --- | --- |
|  17260-35           | 11 - 35**°**C  |