Fully-lugged Lever Operated Butterfly Valve PN16 WRAS Approved

|  |  |
| --- | --- |
| HV-BF-FLL-06 | 2" |
| HV-BF-FLL-07 | 2½" |
| HV-BF-FLL-08 | 3" |
| HV-BF-FLL-09 | 4" |
| HV-BF-FLL-10 | 5" |
| HV-BF-FLL-11 | 6" |
| HV-BF-FLL-12 | 8" |